# GENERAL DESCRIPTION

* 1. The unit shall be an integrated power solution utilizing NightCharge® from Code Blue Corporation, no substitutions, for CB 1 series and CB 4-u product offerings. This shall provide an alternative power option for installations requiring power connectivity to a timed/switched power grid.

# MOUNTING

* 1. The NightCharge power solution shall be mounted internally at the factory and pre-wired for connection of the batteries after physical installation of the units.

# 3rd PARTY PRODUCT SPECIFICATIONS

* 1. ProMariner ProMar 1 Specifications:
     + - **Fully Automatic Charging**: Charges and Conditions batteries with a built-in safe maintenance mode for long and short term storage.
       - **Automatic Charging for Lead or Gel Batteries**: Optimized charging output.
       - **Waterproof and Shock Resistant**: Saltwater tested for coastal areas.
       - **LED Power and Charge Indicators**: At-a-glance power and charging status.

|  |  |
| --- | --- |
| **Electrical Characteristics** | |
| Voltage | 12V |
| Amperage | 5 |
| Banks | 1 |
| AC Input Voltage | 90-135V |
| **Mechanical Characteristics** | |
| Cable Size | 6’ |
| Size | 5.75” L x 3.5” W x 2” H |
| Weight | 5 lbs. |

* 1. MK 8A22NF-Deka Specifications:

|  |  |
| --- | --- |
| **Electrical Characteristics** | |
| Nominal Voltage | 12V |
| Capacity at 100oC | 63 Ah |
| Capacity at 20oC | 55 Ah |
| **Mechanical Characteristics** | |
| Plate Alloy | Lead Calcium |
| Size | 9.72” L x 5.47” W x 9.24” H |
| Weight | 39 lbs |
| Posts | Forged Terminals & Bushings |
| Container/Cover | Polypropylene |
| Vent | Self-sealing |

# WARRANTY

* 1. The NightCharge shall be warrantied against any defects, under normal use, for a period of one year.

# MANUFACTURER

* 1. The Manufacturer shall be Code Blue Corporation. 800-205-7186, 259 Hedcor Street, Holland, Michigan 49423. www.codeblue.com. THERE ARE NO EQUIVALENTS.